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Product Overview
The RG-AP680-CD(V3) is a Wi-Fi 6 wireless access point that delivers dual radios, high performance, and enterprise-grade encryption. Its hybrid cloud management mode and high-density access design allow the RG-AP680-CD(V3) to be flexibly deployed in high-quality outdoor network scenarios, including outdoor hotspots such as squares, parks, and streets in smart cities, sports field scenarios in the education industry, and scenarios related to energy and rail transportation industry.
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Product Highlights
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Ultra-High Performance
Dual-band design (2.4 GHz + 5 GHz), four spatial streams, 1024-Quadrature Amplitude Modulation (QAM) high-speed access, up to 2.976 Gbps peak data rate, and built-in intelligent directional antenna, realizing high-speed wireless access experience
RF power adjustment and intelligent channel allocation to solve the problems such as co-channel interference and adjacent channel interference, thereby improving network transmission efficiency and stability
Flexible Networking
Local and cloud management modes, and intelligent wireless network optimization, reducing TCO and maximizing ROI
Access through optical and Ethernet cables for flexible networking and high-speed backhaul over 2.5 Gbps wired links
Wireless distribution system (WDS) for wireless network coverage or a wireless bridge; high-performance wireless bridging with the distance of 3 km (1.86 miles); point-to-multipoint wireless bridging for the customer-premises equipment (CPE), making wireless networking more flexible
IEEE 802.11k/v/r support and roaming stickiness optimization, achieving seamless user roaming
Rich IoT features: PoE output, Bluetooth 5.0, and wireless locating
High Security and Reliability
IP68 rated housing, adapting to harsh outdoor environments
Encryption and authentication technologies including Wi-Fi Protected Access 3 (WPA3), enhanced open security, 802.1X, and Private Pre-shared Key (PPSK), enhancing data security
Dynamic Frequency Selection (DFS), optimizing the use of available RF spectrum to prevent radar channel interference
Cyclic Delay/Shift Diversity (CDD/CSD), Maximum Ratio Combining (MRC), Space-Time Block Coding (STBC), and Low-Density Parity Check (LDPC), improving the signal quality, signal receiving, and reliability and performance of data transmission
Transmit beam-forming (TxBF) expands the signal coverage and enhances the reliability of specific devices, thereby improving the data rate
Intelligent identification and monitoring, multicast-to-unicast conversion, and other features, enhancing network security and reliability
Applicable Scenarios
Smart City
Parks
With Wi-Fi deployed in parks, people can enjoy high-speed mobile internet access anytime, anywhere. They can flexibly and easily enjoy Internet services, including browsing the web, watching videos, and engaging in voice and video chats with friends.
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Squares
People can access high-speed mobile Wi-Fi and instantly share photos and videos of activities on squares with their friends.
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Higher Education
Sports Field
You can cheer and show support for sports events on the spots field, and share moments in real time on social media. High-speed mobile Wi-Fi allows you to leave real-time memories.
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Note: For more applicable scenarios, contact Ruijie pre-sales engineers.
Product Features
Multi-scenario Adaptability
The RG-AP680-CD(V3), a dual-band wall-mounted wireless access point, is ideal for a wide range of applications, including higher education, government, general education, finance, and business sectors, providing flexible solutions to meet diverse service needs.
High-speed Access and Compatibility
The RG-AP680-CD(V3) supports various wireless protocols, such as 802.11ax, 802.11ac Wave2, 802.11ac Wave1, and 802.11n. It features a hardware-independent dual-band design to deliver a data rate of up to 2.976 Gbps, effectively eliminating wireless performance bottlenecks. Additionally, it is compatible with an extensive array of devices, promoting seamless interconnectivity among employees and customers.
Security and Scalability
The RG-AP680-CD(V3) stands out with its exceptional wireless network security, RF control, mobile access, QoS guarantee, and seamless roaming. With Ruijie's wireless access controller (AC), it enables wireless user data forwarding, security, and access control to cope with diverse service needs.
Flexible Deployment and Power Supply
The RG-AP680-CD(V3) supports both local power supply and Power over Ethernet (PoE), providing you with the flexibility to choose the power supply mode. In addition, the RG-AP680-CD(V3) can be mounted against a wall or pole, making space deployment and environmental requirements less challenging. This makes the RG-AP680-CD(V3) particularly suitable for scenarios such as parks, squares, sports fields, and rail transportation scenarios.
Solution Scalability Capabilities
Ruijie WIS Cloud Management Network Solution (WIS for short, https://wis.ruijienetworks.com/) provides full-lifecycle cloud management network services covering network procurement, planning, deployment, acceptance, and O&M. When the AP connects to WIS, it can meet various needs in multiple scenarios including planning, deployment, acceptance, and operation through cloud management, cloud O&M, cloud authentication, and other value-added services provided by WIS.
Network-wide Cloud Management
WIS supports integrated management and control of various types of devices including APs, ACs, switches, gateways, and routers. It supports remote O&M management operations such as adding or batch importing of multi-branch network devices, online status monitoring, configuration delivery, upgrade, restart, configuration backup, and restoration. It supports network-wide topology auto-discovery and topology status monitoring.
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Wireless Network Visualization
The overview function module of WIS provides a comprehensive view of the network running status from the perspective of overview, experience, users, devices, and environment. The network running information includes the following items:
· Network basic information: device stability, device health, user stability, network signal coverage, and network association.
· User usage: user activity (network dependency), and user online experience and analysis
· Network saturation: network capacity usage and channel usage
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Intelligent Network Diagnosis
With WIS, wireless network diagnosis and health index assessment can be completed in just one click, providing test results for each item. The health index provided by WIS enables you to rapidly assess the state of your live network. WIS can locate faulty areas, APs, and STAs, and provides potential risks and corresponding optimization suggestions.
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Specifications
Hardware Specifications
	Hardware Specifications
	RG-AP680-CD(V3)

	802.11n
	Four spatial streams
Radio 1 – 2.4 GHz: 2x2 MU-MIMO, two spatial streams
Radio 2 – 5 GHz: 4x4 MU-MIMO, two spatial streams
Channels:
Radio 1 – 2.4 GHz: 20 MHz and 40 MHz
Radio 2 – 5 GHz: 20 MHz and 40 MHz
Combined peak data rate: 0.6 Gbps
Radio 1 – 2.4 GHz: 6.5 Mbps to 300 Mbps (MCS0 to MCS15 )
Radio 2 – 5 GHz: 6.5 Mbps to 300 Mbps (MCS0 to MCS15)
Radio technologies: Orthogonal Frequency-Division Multiplexing (OFDM)
Modulation types: BPSK, QPSK, 16-QAM, 64-QAM, 256-QAM
Packet aggregation:
Aggregate MAC Protocol Data Unit (A-MPDU)
Aggregate MAC Service Data Unit (A-MSDU)
Dynamic Frequency Selection (DFS)
Cyclic Delay/Shift Diversity (CDD/CSD)
Maximum Ratio Combining (MRC)
Space-Time Block Coding (STBC)
Low-Density Parity Check (LDPC)
Transmit beam-forming (TxBF)

	802.11ac
	Two spatial streams
Radio 2 – 5 GHz: 2x2 MU-MIMO, two spatial streams
Channels: 
Radio 2 – 5 GHz: 20 MHz, 40 MHz, 80 MHz, and 160 MHz
Combined peak data rate: 1.733 Gbps
Radio 2 – 5 GHz: 6.5 Mbps to 1.733 Gbps (MCS0 to MCS9)
Radio technologies: Orthogonal Frequency-Division Multiplexing (OFDM)
Modulation types: BPSK, QPSK, 16-QAM, 64-QAM, 256-QAM
Packet aggregation:
Aggregate MAC Protocol Data Unit (A-MPDU)
Aggregate MAC Service Data Unit (A-MSDU)
Dynamic Frequency Selection (DFS)
Cyclic Delay/Shift Diversity (CDD/CSD)
Maximum Ratio Combining (MRC)
Space-Time Block Coding (STBC)
Low-Density Parity Check (LDPC)
Transmit beam-forming (TxBF)

	802.11ax
	Four spatial streams
Radio 1 – 2.4 GHz: 2x2 uplink/downlink MU-MIMO, two spatial streams
Radio 2 – 5 GHz: 2x2 uplink/downlink MU-MIMO, two spatial streams
Channels:
Radio 1 – 2.4 GHz: 20 MHz and 40 MHz
Radio 2 – 5 GHz: 20 MHz, 40 MHz, 80 MHz, and 160 MHz
Combined peak data rate: 2.976 Gbps:
Radio 1 – 2.4 GHz: 8.6 Mbps to 0.574 Gbps (MCS0 to MCS11)
Radio 2 – 5 GHz: 8.6 Mbps to 2.402 Gbps (MCS0 to MCS11)
Radio technologies: uplink/downlink Orthogonal Frequency-Division Multiple Access (OFDMA) 
Modulation types: BPSK, QPSK, 16-QAM, 64-QAM, 256-QAM, 1024-QAM
Packet aggregation:
Aggregate MAC Protocol Data Unit (A-MPDU)
Aggregate MAC Service Data Unit (A-MSDU)
Dynamic Frequency Selection (DFS)
Cyclic Delay/Shift Diversity (CDD/CSD)
Maximum Ratio Combining (MRC)
Space-Time Block Coding (STBC)
Low-Density Parity Check (LDPC)
Transmit beam-forming (TxBF)
WPA3

	Antenna
	Wi-Fi
2.4 GHz: two built-in directional antennas, with peak antenna gain of 9 dBi. 
5 GHz: two built-in directional antennas, with peak antenna gain of 9 dBi.
Bluetooth
One integrated vertically polarized omnidirectional antenna, with peak antenna gain of 4.5 dBi. 

	Port
	1 x 2.5GE SFP port, compatibility with 1GE module
1 x 10/100/1000BASE-T port
1 x RJ45 console port (serial console port)
1 x Bluetooth 5.0

	Status LED
	1 x multi-color system status LED
AP power-on status
Software initialization status and upgrade status 
Uplink service interface status
Wireless user online status 
CAPWAP tunnel timeout
Specific AP locating
Three single-color signal strength LEDs:
Whether bridging is enabled
Whether bridging is successful
Wireless signal strength after successful bridging

	Button
	1 x Reset button
Press the button for shorter than 2 seconds. Then the device restarts. 
Press the button for longer than 5 seconds. Then the device restores to factory settings.

	Dimensions (W x D x H)
	Main unit: 251 mm x 168 mm x 64 mm (9.88 in. x 6.61 in. x 2.52 in.)
Shipping: 405 mm x 232 mm x 325 mm (15.94 in. x 9.13 in. x 12.79 in.)

	Weight
	Main unit: 1.5 kg (3.31 lbs) 
Mounting bracket: 0.2 kg (0.44 lbs) 
Shipping: 2.92 kg (6.44 lbs) 

	Mounting
	Wall/Pole-mounting (a mounting bracket is delivered with the main unit)

	Input power supply
	The AP supports the following two power supply modes:
48 V DC/0.35 A power input over DC connector: The DC connector accepts 2.0 mm/6.3 mm center-positive circular plug. A DC power supply needs to be purchased independently. 
PoE input over ETH/PoE: The power source equipment (PSE) complies with IEEE 802.3af/at standard (PoE/PoE+).
Note: If both DC power and PoE are available, DC power is preferred.

	Maximum power consumption
	Maximum power consumption: 12.95 W
DC power: 12.95 W
802.3at (PoE+): 12.95 W
802.3af (PoE): 12.95 W
Idle mode: 6 W

	Environment
	Storage temperature: –40°C to +85°C (–40°F to +185°F)
Storage humidity: 0% RH to 100% RH (non-condensing)
Storage altitude: –500 m to +5,000 m (–1640.42 ft. to +16,404.20 ft.)
Operating temperature: –40°C to +65°C (-40°F to +149°F)
Operating humidity: 0% RH to 100% RH (non-condensing)
Operating altitude: –500 m to +4,000 m (–1,640.42 ft. to +13,123.36 ft.)
Note: At an altitude in the range of 1,800–4,000 m (5,905.51–13,123.36 ft.), every time the altitude increases by 220 m (721.78 ft.), the maximum temperature decreases by 1°C (1.8°F).

	Mean Time Between Failure (MTBF)
	200,000 hours (22 years) at the operating temperature of 25°C (77°F)

	System memory
	512 MB DRAM, 128 MB flash

	Transmit power
	2.4 GHz
Maximum transmit power: 28 dBm (631mW)
Minimum transmit power: 10 dBm (10 mW)
5 GHz
Maximum transmit power: 28 dBm (631mW)
Minimum transmit power: 10 dBm (10 mW)
Note: 
Adjusting the transmit power by percentage (recommended) and in 1dBm increments.
The transmit power is limited by local regulatory requirements. For details, see WLAN Country or Region Codes and Channel Compliance.



The following table lists the radio frequency performance of Wi-Fi including different frequency bands, protocols, and date rates. It is country-specific, and Ruijie Networks reserves the right of interpretation.
	Radio Frequency Performance
	RG-AP680-CD(V3)

	Frequency Band and Protocol
	Data Rate
	Maximum Transmit Power per Transmit Chain
	Maximum Receive Sensitivity per Receive Chain

	2.4 GHz, 802.11b
	1 Mbps
	25 dBm 
	–92 dBm 

	
	2 Mbps
	25 dBm 
	–82 dBm 

	
	5.5 Mbps
	25 dBm
	–84 dBm 

	
	11 Mbps
	25 dBm 
	–78 dBm 

	2.4 GHz, 802.11g
	6 Mbps
	25 dBm
	–84 dBm 

	
	24 Mbps
	23 dBm 
	–74 dBm 

	
	36 Mbps
	23 dBm 
	–72 dBm 

	
	54 Mbps
	20 dBm 
	–67 dBm 

	2.4 GHz, 802.11n (HT20)
	MCS0
	25 dBm 
	–84 dBm 

	
	MCS7
	20 dBm 
	–66 dBm 

	2.4 GHz, 802.11n (HT40)
	MCS0
	25 dBm 
	–79 dBm 

	
	MCS7
	20 dBm 
	–63 dBm 

	2.4 GHz, 802.11ax (HE20)
	MCS0
	25 dBm 
	–84dBm 

	
	MCS11
	18 dBm 
	–54 dBm 

	2.4 GHz, 802.11ax (HE40)
	MCS0
	25 dBm 
	–80 dBm 

	
	MCS11
	18 dBm 
	–51 dBm 

	5 GHz, 802.11a
	6 Mbps
	25 dBm 
	–84 dBm 

	
	24 Mbps
	23 dBm 
	–74 dBm 

	
	36 Mbps
	23 dBm 
	–72 dBm 

	
	54 Mbps
	20 dBm 
	–67 dBm 

	5 GHz, 802.11n (HT20)
	MCS0
	25 dBm 
	–84 dBm 

	
	MCS7
	20 dBm 
	–66 dBm 

	5 GHz, 802.11n (HT40)
	MCS0
	25 dBm 
	–81 dBm 

	
	MCS7
	20 dBm 
	–63 dBm 

	5 GHz, 802.11ac (VHT20)
	MCS0
	25 dBm 
	–84 dBm 

	
	MCS9
	19 dBm 
	–61 dBm 

	5 GHz, 802.11ac (VHT40)
	MCS0
	25 dBm 
	–81 dBm 

	
	MCS9
	19 dBm 
	–56 dBm 

	5 GHz, 802.11ac (VHT80)
	MCS0
	25 dBm 
	–78 dBm 

	
	MCS9
	19 dBm 
	–53 dBm 

	5 GHz, 802.11ax (HE20)
	MCS0
	25 dBm 
	–84 dBm 

	
	MCS11
	18 dBm 
	–54 dBm 

	5 GHz, 802.11ax (HE40)
	MCS0
	25 dBm 
	–81 dBm 

	
	MCS11
	18 dBm 
	–51 dBm 

	5 GHz, 802.11ax (HE80)
	MCS0
	25 dBm 
	–78 dBm 

	
	MCS11
	18 dBm 
	–48 dBm 

	5 GHz, 802.11ax (HE160)
	MCS0
	25 dBm 
	–73 dBm 

	
	MCS11
	18 dBm 
	–43 dBm 



Note: Available frequency bands may vary with countries or regions. To use the above-mentioned frequency bands, ensure that they are supported in your country or region. For details, see WLAN Country or Region Codes and Channel Compliance.
Software Specifications
Basic Functions
	Basic Function
	RG-AP680-CD(V3)

	Applicable software version
	RGOS11.9(6)W2B4 or later

	WLAN
	

	Maximum number of associated STAs
	1024 (up to 512 STAs per radio)

	Practical maximum client count indication (per device)
	128

	Maximum number of BSSIDs
	32 (up to 16 BSSIDs per radio)

	Maximum number of WLAN IDs
	16

	STA management
	SSID hiding
Band steering
Each SSID can be configured with the authentication mode, encryption mechanism, and VLAN attributes independently.
Remote Intelligent Perception Technology (RIPT)
Intelligent load balancing based on the STA quantity or traffic
Rate set settings
Intelligent STA identification

	STA limiting
	SSID-based STA limiting
Radio-based STA limiting

	Bandwidth limiting
	STA/SSID/AP-based rate limiting

	CAPWAP
	IPv4/IPv6 CAPWAP
Layer 2 and Layer 3 topology between an AP and an AC
An AP can automatically discover the accessible AC.
An AP can be automatically upgraded through the AC.
An AP can automatically download the configuration file from the AC.
CAPWAP through NAT 

	Data forwarding
	Centralized and local forwarding

	Wireless roaming
	Layer 2 and Layer 3 roaming

	Wireless locating
	MU and TAG device locating

	Application management
	Application identification

	Security and Authentication
	

	Authentication and encryption
	Remote Authentication Dial-In User Service (RADIUS)
EXEC authorization, specifying the source IP address of RADIUS packets, and built-in authentication server 
PSK, UPSK and web authentication
QR code-based guest authentication, SMS authentication, and MAC address bypass (MAB) authentication
Data encryption: WEP (64/128 bits), WPA-Personal, WPA-Enterprise, WPA2-Personal (PSK, TKIP, CCMP), WPA2-Enterprise, WPA3-Personal (SAE, WPA2/WPA3 transition mode), WPA3-Enterprise (CCMP)

	Data frame filtering
	Allowlist, static blocklist, and dynamic blocklist

	WIDS
	Wireless Intrusion Detection System(WIDS)
Wireless Intrusion Protection System(WIPS)
User isolation
Rogue AP detection and containment

	Dynamic Policy
	IP standard ACL, MAC extended ACL, IP extended ACL, and expert-level ACL
IPv6 ACL
Time range-based ACL
ACL based on a Layer 2 interface
ACL based on a Layer 3 interface
Ingress ACL based on a wireless interface
Dynamic ACL assignment based on 802.1X authentication (used with the AC)
CoA/DM
ACL REMARK

	CPP
	CPU Protect Policy (CPP)

	NFPP
	Network Foundation Protection Policy (NFPP)

	Routing and Switching
	

	MAC
	Static and filtered MAC addresses
MAC address table size: 1,024
Maximum number of static MAC addresses: 1,024
Maximum number of filtered MAC addresses: 1,024

	Ethernet
	Jumbo frame length: 1518
Full-duplex and half-duplex modes of interfaces 
IEEE802.1p and IEEE802.1Q

	VLAN
	Interface-based VLAN assignment
Maximum number of SVIs: 200
Maximum number of VLANs: 4,094
VLAN ID range: 1–4,094

	ARP
	ARP entry aging, gratuitous ARP learning, and proxy ARP
Maximum number of ARP entries: 1,024
ARP check

	IPv4 services
	Static and DHCP-assigned IPv4 addresses
NAT, FTP ALG and DNS ALG

	IPv6 services
	IPv6 addressing, Neighbor Discovery (ND), ICMPv6, IPv6 ping
IPv6 DHCP client

	IP routing
	IPv4/IPv6 static route
Maximum number of static IPv4 routes: 1,024
Maximum number of static IPv6 routes: 1,000

	Multicast
	Multicast-to-unicast conversion

	VPN
	PPPoE client
IPsec VPN

	Network Management and Monitoring
	

	Network management
	NTP server and NTP client
SNTP client
SNMPv1/v2c/v3
Fault detection and alarm
Information statistics and logging

	Network management platform
	Web management (Eweb)

	User access management
	Telnet, SSH, FTP client, and FTP management

	Switchover among Fat, Fit, and cloud modes
	When the AP works in Fit mode, it can be switched to Fat mode through an AC.
When the AP works in Fat mode, it can be switched to Fit mode through the console port or Telnet mode.
When the AP works in cloud mode, it can be managed through WIS Cloud.



Value-added Software
The following value-added software functions can be achieved with the WIS solution (used with RG-iData-WIS and wireless controller). 
	Value-added Software
	RG-AP680-CD(V3)

	Intelligent O&M
	

	Experience
	Network operation analysis, such as device stability and signal coverage
Measuring users' network experience based on indicators such as the latency, packet loss, signal strength, and channel utilization, and visualizing results of the network experience
Statistics on the number of online and offline failures of STAs associated with different APs, average signal strength, and other parameters
VIP monitoring and alarm, and custom alarm thresholds
STA global experience map and experience coverage evaluation based on the time range
STA access protocol replay and fine-grained STA fault diagnosis
Note: To support the preceding functions, ensure that the AP works in Fit mode.

	Network optimization
	Network performance optimization, including one-click network optimization and scenario-based optimization
Client steering to cope with roaming stickiness, and experience indicator comparison
Client steering to cope with remote association, and experience indicator comparison
One-click diagnosis – analyzing problems and providing suggestions

	Big data
	Baseline analysis – recording the configuration, version, and other changes, and tracking network KPI changes
Time capsule – analyzing the device version and configuration change history

	Regional analysis
	Batch generation of building floor information – uploading floor plans, and dragging and dropping AP positions

	One-click report
	One-click health report – generating a report on the overall operation of a network

	Security radar
	Unauthorized Wi-Fi signal location, presentation by category, and containment

	Cloud Management
	

	Management and maintenance
	Uniformly connecting, managing, and maintaining APs, ACs, and other devices, batch device configuration and upgrade, and other functions
Deployment through Zero Touch Provisioning (ZTP) – creating configuration templates and automatically applying configured templates
One-click discovery of the wired and wireless network topology and topology generation

	Cloud Authentication
	

	Authentication mode
	SMS authentication, fixed account authentication, one-click authentication, Facebook authentication, Instagram authentication, voucher authentication, and other authentication modes
Authentication implemented in the cloud, without the need to deploy the local authentication server

	Customized portal
	Customized Portal authentication page for mobile phones and PCs

	SMS gateway
	Interconnection with SMS gateways of GUODULINK and Alibaba Cloud

	Platform Capabilities
	

	Big data capabilities
	Mainstream persistence solutions based on Hadoop, MongoDB, and MySQL, providing distributed storage capabilities
Spark-based big data computing capabilities
Data warehouse building based on Hive, and data model conversion, integration, and other functions

	Hierarchy and decentralization
	Authorizing different applications for different users to meet service needs of different departments
Granting operation permissions to administrators in different scenarios

	System management
	Account operation, authorization configuration, email configuration, configuration backup, exception alarms, and other system management functions


Note: For details, refer to the latest hybrid cloud management solution.

Regulatory Compliance
	Regulatory Compliance
	RG-AP680-CD(V3)

	Regulatory compliance
	EN 55032, EN 55035, EN 61000-3-3, EN IEC 61000-3-2, EN 301 489-1, EN 301 489-3, EN 301 489-17, EN 300 328, EN 301 893, EN 300 440, FCC Part 15, EN 62311, EN IEC 62311, IEC 62368-1, EN 50665, EN 62368-1, IEC 60950-22, EN 18031-1, and EN 18031-2


* For more country-specific regulatory information and approvals, contact your local sales agency.
Note：
EU simplified DoC: Hereby, [Ruijie Networks Co., Ltd.] declares that the radio equipment type [RG-AP680-CD(V3)] is in compliance with Directive 2014/53/EU. The full text of the EU declaration of conformity is available at the following internet address: https://www.ruijie.com/.
UK simplified DoC: Hereby, [Ruijie Networks Co., Ltd.] declares that the radio equipment type [RG-AP680-CD(V3)] is in compliance with UK Radio Equipment Regulation 2017. The full text of the UK declaration of conformity is available at the following internet address: https://www.ruijie.com/.
The functions of Wireless Access Systems including Radio Local Area Networks(WAS/RLANs) within the band 5150-5350 MHz for this device are restricted to indoor use only within all European Union countries (BE/BG/CZ/DK/DE/EE/IE/EL/ES/FR/HR/IT/CY/LV/LT/LU/HU/MT/NL/ AT/PL/PT/RO/SI/SK/FI/SE/TR/NO/CH/IS/LI/UK(NI)
[image: E:\RjDir\admin_d95c8884-f44c-4529-8f3b-48d5788371c1\Documents\WeChat Files\wxid_op7d6uqpyrcs22\FileStorage\Temp\706548e633bb6401b722b743cc41ba1.png][image: E:\RjDir\admin_d95c8884-f44c-4529-8f3b-48d5788371c1\Documents\WeChat Files\wxid_op7d6uqpyrcs22\FileStorage\Temp\ebf0007d0040df2fc4874e152b98a1c.png]

Ruijie wireless products provide only secure and reliable network protocols and communication ports by default. For details, see Ruijie Default Protocols and Ports for Wireless Products. Proper firewall and security policies can be implemented based on this document to ensure the normal operation of wireless services.
Antenna Pattern Plots
Horizontal Planes (Top View)
The following figures show the azimuth antenna pattern at 2.4 GHz and 5 GHz radios.
[image: ] [image: ]

Vertical Planes (Side View, AP Facing Down)
The following figures shows the elevation antenna pattern at 2.4 GHz and 5 GHz radios.
[image: ] [image: ]
Note: Operating frequency bands are country-specific.
Ordering Information
	Model
	Description

	RG-AP680-CD(V3)
	802.11ax-compliant outdoor high-density wireless access point
Dual radios, four spatial streams, peak data rate of 2.976 Gbps
Radio 1: 2.4 GHz: two spatial streams, 2x2 MU-MIMO, peak data rate of 574 Mbps
Radio 2: 5 GHz: two spatial streams, 2x2 MU-MIMO, peak data rate of 2.402 Gbps
802.11a/b/g/n/ac/ax, switching between Fat, Fit, and cloud modes, and 802.3af/at PoE and local DC power supply
Note:
The power source equipment (PSE) needs to be purchased separately.
The DC power supply needs to be purchased separately, and the output voltage/current must be 48 V/0.35 A.



[bookmark: _Toc106024150][bookmark: _Toc107841105][bookmark: _Toc129271575]Package Contents
	Item
	Quantity

	RG-AP680-CD(V3) AP
	1

	Mounting bracket
	1

	Support for pole-mounted or wall-mounted installation
	1

	Machine tooth screw M5 x 10 mm
	4

	Machine tooth screw M6 x 20 mm
	2

	M6 x 50 expansion bolt
	4

	Waterproof PG head
	2

	Fiber cable waterproof connector
	1

	Metal hook
	2

	Grounding cable
	1

	Warranty Card and Hazardous Substance Table
	1

	Hardware Installation Manual
	1

	Dustproof cover
	3

	Ruijie wireless product management software (pre-installed on the AP)
	1


Warranty
For more information about warranty terms and period, contact your local sales agency:
Warranty terms: https://www.ruijie.com/support/servicepolicy
Warranty period: https://www.ruijie.com/support/servicepolicy/Service-Support-Summany/
Note: The warranty terms are subject to the terms of different countries and distributors.
More Information
For more information about Ruijie Networks, visit the official Ruijie website or contact your local sales agency:
Ruijie Networks official website: https://www.ruijie.com/
Online support: https://www.ruijie.com/support
Hotline support: https://www.ruijie.com/support/hotline 
Email support: EBGITSC@ruijie.com.cn
WLAN Country or Region Codes and Channel Compliance: https://www.ruijie.com/support/documents/slide_wlan-country-codes-overview
Ruijie Default Protocols and Ports for Wireless Products: https://www.ruijie.com/en-global/support/documents/slide_wlan-network-protocol-port/
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